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[bookmark: section_1_product_hero]SECTION 1 — PRODUCT HERO
[H1 — Benefit-led, sentence case, left-aligned, semi-bold]
Vanguard 12,000 BTU mini split | 24 SEER2 | Wi-Fi | Up to 750 sq. ft.       
[Star rating widget — placeholder]
[Rating widget: pull from review system]

[Short product descriptor — body copy, 2 sentences]
Year-round heating and cooling for living rooms, master bedrooms, and open-plan spaces. Whisper-quiet, energy-smart, and built to perform even when outdoor temperatures drop to -13°F.

[3 feature hook bullets — displayed prominently beneath descriptor]
· Heats down to -13°F — where most mini splits give up
· 24 SEER2 — among the highest efficiency ratings in this class
· 30 dB(A) quiet — quieter than a library whisper

[CTA button — sentence case, semi-bold]
Find a retailer

[Model ID — small/muted text beneath CTA]
Model: SAC12SNV23-1

[bookmark: section_2_feature_benefit_cards]SECTION 2 — FEATURE BENEFIT CARDS
[Section H2 — benefit-led, sentence case, semi-bold]
Built for better living, every season
[Section subheading — body copy]
Every feature in the Vanguard is designed to make your home more comfortable, more efficient, and healthier — without adding complexity to your life.

[Feature card 1 — icon: snowflake/flame]
[bookmark: reliable_heat_when_it_matters_most]Reliable heat when it matters most
While most mini splits struggle in deep winter, the Vanguard keeps delivering — 8,900 BTU at 5°F, 7,800 BTU at 17°F. Heating mode operates down to -13°F, so your living space stays warm through the coldest nights.

[Feature card 2 — icon: leaf/energy]
[bookmark: lower_energy_bills_every_single_month]Lower energy bills, every single month
At 24 SEER2 — among the highest efficiency ratings in this category — the Vanguard draws measurably less power than competing 12,000 BTU units rated at 19–21.5 SEER2. Energy Star and AHRI certified, so the savings are real, not estimated.

[Feature card 3 — icon: sound wave]
[bookmark: a_home_that_stays_peaceful]A home that stays peaceful
30 dB(A) indoor operation — quieter than most room AC units. Whether you're entertaining, working, or winding down, you'll notice the comfort before you notice the unit.

[Feature card 4 — icon: smartphone/wifi]
[bookmark: control_your_climate_from_anywhere]Control your climate from anywhere
Adjust temperature, set schedules, and switch modes from your smartphone. Works with Alexa and Google Assistant for hands-free voice control. A backlit remote with 24-hour timer means it works without Wi-Fi too.

[Feature card 5 — icon: sparkle/clean]
[bookmark: cleaner_air_without_the_maintenan_b39b62]Cleaner air, without the maintenance headaches
High-temp self-clean heats the coil to sterilizing temperature, eliminating mold and bacteria at the source — no service call required. Filter change alerts and built-in self-diagnosis keep everything running at its best.

[Feature card 6 — icon: box/toolset]
[bookmark: ready_to_install_nothing_left_to_source]Ready to install. Nothing left to source.
Ships complete with a 25 ft pre-charged line set, wall mounting bracket, outdoor pad, and washable dust filter. No refrigerant tank needed on site. Professional installation required.

[bookmark: section_3_features_icon_grid]SECTION 3 — FEATURES ICON GRID
[Section H2 — semi-bold, sentence case]
Thoughtfully engineered, inside and out
[Section subheading — body copy]
Thoughtfully designed features that deliver superior comfort, cleaner air, and smarter performance for your home.

[Icon grid — 2 or 3 columns. Each item: icon + bold label + short descriptor]
	Feature
	Descriptor

	Inverter compressor
	Energy-saving, stable temperatures

	24 SEER2
	Among the highest efficiency ratings in its class

	R32 refrigerant
	Lower environmental impact than R410A

	8 comfort modes
	Auto, Cool, Heat, Dry, Fan, Turbo, Sleep, Eco

	4-way auto swing
	Even airflow in every direction

	iFeel / Follow Me
	Adjusts to where you are in the room

	Wi-Fi + app control
	Manage comfort from anywhere

	Alexa & Google Assistant
	Hands-free voice control

	High-temp self-clean
	Automatic coil sterilization

	Refrigerant leak detector
	Built-in safety protection

	Chassis heater
	Cold climate reliability

	Modular PCB design
	Easier servicing, longer life

	Backlit remote
	24-hour timer — no Wi-Fi needed

	Top-access washable filter
	Simple upkeep, no tools required

	Auto restart
	Resumes after power interruptions

	5-year compressor warranty
	Built to outlast the competition




[bookmark: section_4_product_technical_speci_2b2ca3]SECTION 4 — PRODUCT TECHNICAL SPECIFICATIONS
[Section H2 — semi-bold, sentence case]
Product technical specifications
[Section subheading — body copy]
Full performance, installation, and dimensional details for the Vanguard SAC12SNV23-1.

[Downloads — with download icon/button]
· User manual [Download]
· Product dimensions sheet [Download]

[bookmark: core_performance]Core performance
	Specification
	Value

	Cooling capacity
	12,000 BTU (range: 2,500–12,500 BTU)

	Heating capacity
	12,400 BTU (range: 2,500–15,000 BTU)

	Heating capacity @ 5°F
	8,900 BTU

	Heating capacity @ 17°F
	7,800 BTU

	Cold climate operation
	Down to -13°F

	SEER2
	24

	EER2 @ 95°F
	13

	HSPF
	10

	Coverage area
	Up to 750 sq ft

	Inverter
	Yes

	Zone
	Single zone

	Moisture removal
	1.4 L/h



[bookmark: comfort_acoustics]Comfort & acoustics
	Specification
	Value

	Indoor noise level
	46 / 44 / 36 / 32 / 30 dB(A)

	Outdoor noise level
	56 dB(A)

	Airflow (Low / Med / High)
	323 / 411 / 470 CFM

	Operating modes
	Auto, Cool, Heat, Dry, Fan-Only, Turbo, Sleep, Eco

	Auto swing
	4-way (up/down + left/right)

	iFeel / Follow Me
	Yes

	Louver position memory
	Yes

	Frost protection
	46°F (8°C)

	Set point temperature range
	60.8°F – 87.8°F



[bookmark: energy_refrigerant]Energy & refrigerant
	Specification
	Value

	Energy Star certified
	Yes

	AHRI certified
	Yes

	Refrigerant
	R32

	Refrigerant charge
	27.2 oz

	Additional charge rate
	0.56 oz/ft



[bookmark: installation_electrical]Installation & electrical
	Specification
	Value

	Voltage
	115V

	Rated input power (cooling)
	920W

	Rated input power (heating)
	920W

	Rated current (cooling)
	8A

	Rated current (heating)
	8A

	Minimum circuit ampacity
	10A

	Maximum overcurrent protection
	15A

	Pre-charged line set
	25 ft

	Maximum lineset length
	49 ft

	Maximum elevation difference
	33 ft

	Connecting pipe — gas line
	3/8"

	Connecting pipe — liquid line
	1/4"

	Connecting wiring
	4 × 16AWG

	Estimated installation time
	~2 hours

	Condensate drain method
	Gravity



[bookmark: dimensions_weight]Dimensions & weight
	
	Indoor unit (IDU)
	Outdoor unit (ODU)

	Dimensions (W × D × H)
	36-1/4" × 7-5/8" × 12"
	31-1/2" × 12" × 21-3/4"

	Net weight
	22.0 lbs
	58.0 lbs

	Gross weight
	28.6 lbs
	64.5 lbs



[bookmark: smart_connectivity]Smart & connectivity
	Specification
	Value

	Wi-Fi app control
	Yes

	Local on-device scheduling
	Yes

	Alexa
	Yes

	Google Assistant
	Yes

	Apple HomeKit
	No

	Geofencing
	No

	Filter change alert
	Yes

	Self-diagnosis
	Yes

	Timer
	Yes

	Display on/off
	Yes

	°C / °F switch
	Yes



[bookmark: hygiene_maintenance]Hygiene & maintenance
	Specification
	Value

	Self-clean
	Yes

	High-temp self-clean & sterilization
	Yes

	Deep-clean air channel
	Yes

	Filter type
	Washable (top-access)



[bookmark: reliability_assurance]Reliability & assurance
	Specification
	Value

	Compressor warranty
	5 years

	Parts warranty
	1 year

	Registration required
	No

	Coil anti-corrosion coating
	Yes

	Refrigerant leak detector
	Yes

	Chassis heater (cold climate)
	Yes

	Fire-rated electrical box
	Yes

	Modular PCB design
	Yes

	Advanced defrost logic
	Yes

	Auto restart
	Yes

	Forced defrost
	Yes



[bookmark: compressor]Compressor
	Specification
	Value

	Compressor brand
	GMCC

	Compressor type
	Rotary

	Compressor model
	KSN98D31UEZA31




[bookmark: section_5_you_may_also_like]SECTION 5 — YOU MAY ALSO LIKE
[Section H2 — semi-bold, sentence case]
Explore the full Vanguard series
[3 product cards. Each card: product name, descriptor, price, CTA button]

[Product card 1]
Electrolux Vanguard 9,000 BTU
Single-zone mini split | 23 SEER2 | Up to 450 sq ft | 115V
$1,079
[View product]

[Product card 2]
Electrolux Vanguard 18,000 BTU
Single-zone mini split | 24 SEER2 | Up to 1,000 sq ft | 208/230V
$1,599
[View product]

[Product card 3]
Electrolux Vanguard 24,000 BTU
Single-zone mini split | 23 SEER2 | Up to 1,250 sq ft | 208/230V
$1,949
[View product]

[bookmark: section_6_customer_reviews]SECTION 6 — CUSTOMER REVIEWS
[Section H2 — semi-bold, sentence case]
What homeowners are saying
[Reviews widget — placeholder for live review integration. Display: aggregate star rating, total review count, star breakdown, individual reviews with verified buyer badge]
[Reviews widget placeholder]

[bookmark: section_7_brand_promise_sign_off]SECTION 7 — BRAND PROMISE SIGN-OFF
[Semi-bold, sentence case — required on all product pages per brand guidelines]
For better living. From Sweden.

[bookmark: section_8_email_newsletter_sign_up]SECTION 8 — EMAIL NEWSLETTER SIGN-UP
[Section heading — H2, semi-bold, sentence case]
Stay ahead of home comfort
[Body copy]
Get the latest from Electrolux — tips, updates, and exclusive offers delivered to your inbox.
[Input field placeholder text]
Your email address
[CTA button — sentence case, semi-bold]
Subscribe

[bookmark: designer_notes]DESIGNER NOTES
1. Spec tables should use a collapsible accordion format by category (Core Performance, Comfort & Acoustics, etc.) — same structure as SAC09SNV23-1
2. "Find a retailer" CTA appears in the hero (Section 1) and as a sticky/floating button visible on scroll
3. Key differentiator vs. the 9K model: This unit is 24 SEER2 (vs. 23), covers 750 sq ft (vs. 450), and has higher airflow (323/411/470 CFM vs. 188/235/282 CFM) — ensure these are visually prominent
4. Voltage is still 115V — same as the 9K model. The 208/230V step-up begins with the 18K and 24K models
5. Brand promise ("For better living. From Sweden.") must appear as semi-bold sentence case — never uppercase, never locked with the logo
6. CTAs throughout are sentence case — never all caps
7. Professional installation is required — retain this disclosure in the hero bullets and installation card
